Amplificateur Yamaha

Liste des commandes dans calaos installer

Fonctionne avec la serie rx

Volume X

Power on

Power off

source X

source 1 -> HDMI 1
source 2 -> HDMI 2
source 3 -> HDMI 3
source 4 -> HDMI 4
source 5 -> HDMI 5
source 6 -> Tuner
source 7 -> Phono
source 8-> Video 1
source 9 -> Video 2
source 10 -> Video 3
source 11 -> Video 4
source 12 -> Video 5
source 13 -> Video 6
source 14 -> V-Aux
source 15 -> Audio 1
source 16 -> Audio 2
source 17 -> Dock
source 18 -> iPod
source 19 -> Bluetooth
source 20 -> Network
source 21 -> Napster
source 22 -> Net Radio
source 23 -> USB
source 24-> iPod (USB)
source 25 -> PC
source 26 -> UAW

custom cmd

exemple

custom @MAIN:INP=HDMI1

@MAIN @ZONE2 @ZONE3

Command Details of SubUnit: MAIN
PWR
[PUT Command]
**@MAIN:PWR=**
[Parameters]
**Standby**
PUT: turining its state to Standby / GET: indicating Standby status.
**On**
PUT: turining its state to On / GET: indicating On status.
**On/Standby**
PUT Only: toggling its status between On/Standby
SLEEP
[PUT Command]
**@MAIN:SLEEP=**
[Parameters]
**Off**
PUT: turining its setting state to Off / GET: indicating Off setting status.
**30 min**
PUT: setting to 30 min / GET: indicating it's setting is 30 min.
**60 min**
PUT: setting to 60 min / GET: indicating it's setting is 60 min.
**90 min**
PUT: setting to 90 min / GET: indicating it's setting is 90 min.
**120 min**
PUT: setting to 120 min / GET: indicating it's setting is 120 min.
**Last**
PUT Only: setting to the value set last
**VOL**
[PUT Command]
**@MAIN:VOL=**
[Parameters]
**Down**
PUT Only: decrementing by 1 step (0.5dB)
**Up**
PUT Only: incrementing by 1 step (0.5dB)
**Down 1 dB**
PUT Only: decrementing by 1 dB
Up 1 dB
PUT Only: incrementing by 1 dB
Down 2 dB
PUT Only: decrementing by 2 dB
Up 2 dB
PUT Only: incrementing by 2 dB
Down 5 dB
PUT Only: decrementing by 5 dB
Up 5 dB
PUT Only: incrementing by 5 dB
Numerical Number: -80.5 to 16.5, Step: 0.5
PUT: setting to the specified value. / GET: indicating the current value.
-80.5 means muting. First decimal place must be always included. Ex: 10.0, -25.0 or 0.0 etc.
The unit for this parameter is "dB".
**MUTE**
[PUT Command]
**@MAIN:MUTE=**
[Parameters]
**Off****Bold Text**
PUT: turining its state to Off / GET: indicating Off status.
**Att -40 dB**
PUT: attenuating by 40 dB from current volume status. / GET: indicating attenuated by 40 dB from current
volume status.
Att -20 dB
PUT: attenuating by 20 dB from current volume status. / GET: indicating attenuated by 20 dB from current
volume status.
On
PUT: turining its state to On / GET: indicating On status.
On/Off
PUT Only: toggling its status between On/Off
MAXVOL
[PUT Command]
@MAIN:MAXVOL=
[Parameters]
Numerical Number: -30.0 to 15.0, Step: 5.0
PUT: setting to the specified value. / GET: indicating the current setting value.
First decimal place must be always included. Ex: 10.0, -25.0 or 0.0 etc.
The unit for this parameter is "dB".
16.5
PUT: setting to the specified value. / GET: indicating the current setting value.
Meaning no limit of maximum volume
The unit for this parameter is "dB".
INITVOLMODE
[PUT Command]
@MAIN:INITVOLMODE=
[Parameters]
Off
PUT: turining its setting state to Off / GET: indicating Off setting status.
On
PUT: turining its setting state to On / GET: indicating On setting status.
INITVOLLVL
[PUT Command]
@MAIN:INITVOLLVL=
[Parameters]
Mute
PUT: turining its setting state to Mute / GET: indicating Mute setting status.
Initially muted when turned on
Numerical Number: -80.0 to 16.5, Step: 0.5
PUT: setting to the specified value. / GET: indicating the current setting value.
First decimal place must be always included. Ex: 10.0, -25.0 or 0.0 etc.
The unit for this parameter is "dB".
INP
[PUT Command]
@MAIN:INP=
[Parameters]
SIRIUS
PUT: selecting input SIRIUS / GET: indicating current input is SIRIUS
TUNER
PUT: selecting input TUNER / GET: indicating current input is TUNER
HDMI1
PUT: selecting input HDMI1 / GET: indicating current input is HDMI1
HDMI2
PUT: selecting input HDMI2 / GET: indicating current input is HDMI2
HDMI3
PUT: selecting input HDMI3 / GET: indicating current input is HDMI3
HDMI4
PUT: selecting input HDMI4 / GET: indicating current input is HDMI4
HDMI5
PUT: selecting input HDMI5 / GET: indicating current input is HDMI5
AV1
PUT: selecting input AV1 / GET: indicating current input is AV1
AV2
PUT: selecting input AV2 / GET: indicating current input is AV2
AV3
PUT: selecting input AV3 / GET: indicating current input is AV3
AV4
PUT: selecting input AV4 / GET: indicating current input is AV4
AV5
PUT: selecting input AV5 / GET: indicating current input is AV5
AV6
PUT: selecting input AV6 / GET: indicating current input is AV6
V-AUX
PUT: selecting input V-AUX / GET: indicating current input is V-AUX
AUDIO1
PUT: selecting input AUDIO1 / GET: indicating current input is AUDIO1
AUDIO2
PUT: selecting input AUDIO2 / GET: indicating current input is AUDIO2
DOCK
PUT Only: selecting input DOCK
iPod
PUT: selecting input iPod / GET: indicating current input is iPod
Bluetooth
PUT: selecting input Bluetooth / GET: indicating current input is Bluetooth
UAW
PUT: selecting input UAW / GET: indicating current input is UAW
NET
PUT Only: selecting input NET
Rhapsody
PUT: selecting input Rhapsody / GET: indicating current input is Rhapsody
SIRIUS InternetRadio
PUT: selecting input SIRIUS InternetRadio / GET: indicating current input is SIRIUS InternetRadio
Pandora
PUT: selecting input Pandora / GET: indicating current input is Pandora
Napster
PUT: selecting input Napster / GET: indicating current input is Napster
PC
PUT: selecting input PC / GET: indicating current input is PC
NET RADIO
PUT: selecting input NET RADIO / GET: indicating current input is NET RADIO
USB
PUT Only: selecting input USB
iPod (USB)
PUT: selecting input iPod (USB) / GET: indicating current input is iPod (USB)
DECODERSEL
[PUT Command]
@MAIN:DECODERSEL=
[Parameters]
Auto
PUT: turining its setting state to Auto / GET: indicating Auto setting status.
Automatically selects audio decoder. Default value.
DTS
PUT: turining its setting state to DTS / GET: indicating DTS setting status.
Audio decoder is fixed to DTS
Unavailable
GET Only: indicating its setting is currently unavailable.
SCENE
[PUT Command]
@MAIN:SCENE=
[Parameters]
Scene 1
PUT Only: selecting Scene 1
Scene 2
PUT Only: selecting Scene 2
Scene 3
PUT Only: selecting Scene 3
Scene 4
PUT Only: selecting Scene 4
SPBASS
[PUT Command]
@MAIN:SPBASS=
[Parameters]
Numerical Number: -6.0 to 6.0, Step: 0.5
PUT: setting to the specified value. / GET: indicating the current setting value.
First decimal place must be always included. Ex: 3.0, -4.0
The unit for this parameter is "dB".
SPTREBLE
[PUT Command]
@MAIN:SPTREBLE=
[Parameters]
Parameters are the same as
SPBASS
PUREDIRMODE
[PUT Command]
@MAIN:PUREDIRMODE=
[Parameters]
Off
PUT: turining its setting state to Off / GET: indicating Off setting status.
On
PUT: turining its setting state to On / GET: indicating On setting status.
ADAPTIVEDRC
[PUT Command]
@MAIN:ADAPTIVEDRC=
[Parameters]
Off
PUT: turining its setting state to Off / GET: indicating Off setting status.
Auto
PUT: turining its setting state to Auto / GET: indicating Auto setting status.
LIPSYNCMODE
[PUT Command]
@MAIN:LIPSYNCMODE=
[Parameters]
Manual
PUT: turining its setting state to Manual / GET: indicating Manual setting status.
About "Manual" setting of Lipsync Mode: When selecting "Manual" here, the audio delay value can be
manually set. The effective setting of the audio delay value has some dependencies as follows. In case of
using Analog Video Output only (no HDMI connection is active), audio delay value set by "@MAIN:ANLGOUT"
command is effective. In case that HDMI OUT1 is in active connection, the value set by
"@MAIN:HDMIOUT1MANUAL" command works. Else if HDMI OUT2 is the only one activated, the setting by
"@MAIN:HDMIOUT2MANUAL" is enabled.
Auto
PUT: turining its setting state to Auto / GET: indicating Auto setting status.
About Lipsync Mode "Auto": Basically, Audio Delay value has 5 different settings internally according to "Video
Output State (5 Status available)". And the 5 different status of "Video Output State" is determined by the
combination of two states of "Display's state of compatibility/incompatibility with Auto Lipsync feature" and
"Current effective HDMI output state (on the receiver)", which means 4 status, plus a status of "Analog Video
Out only in use", summing up to 5 in total. The "Auto" setting of Lipsync Mode is to dynamically change the
Audio Delay value corresponding to a specific status of Video Output State. "Video Output State" can be
retrieved with a command of "@MAIN:SELINFO", and you can set the effective Audio Delay value according to
respective Video Output status by these commands as following;
When "@MAIN:SELINFO=Analog": the audio delay can be set by "@MAIN:ANLGOUT" command
When "@MAIN:SELINFO=HDMI1 Auto" (meaning TV compatible with Auto Lipsync and HDMI OUT1 is
effective): the audio delay can be set by "@MAIN:HDMIOUT1OFFSET" command
When "@MAIN:SELINFO=HDMI1 Manual" (meaning TV incompatible with Auto Lipsync and HDMI OUT1 is
effective): the audio delay can be set by "@MAIN:HDMIOUT1MANUAL" command
When "@MAIN:SELINFO=HDMI2 Auto" (meaning TV compatible with Auto Lipsync and HDMI OUT 2 is the
only one in effective): the audio delay can be set by "@MAIN:HDMIOUT2OFFSET" command
When "@MAIN:SELINFO=HDMI2 Manual" (meaning TV incompatible with Auto Lipsync and HDMI OUT 2 is
the only one in effective): the audio delay can be set by "@MAIN:HDMIOU21MANUAL" command
LIPSYNCANLGOUT
[PUT Command]
@MAIN:LIPSYNCANLGOUT=
[Parameters]
Down
PUT Only: incrementing by 1 step (1 millisecond)
Up
PUT Only: decrementing by 1 step (1 millisecond)
Numerical Number: 0 to 250, Step: 1
PUT: setting to the specified value. / GET: indicating the current value.
The unit for this parameter is "ms".
LIPSYNCHDMIOUT1OFFSET
[PUT Command]
@MAIN:LIPSYNCHDMIOUT1OFFSET=
[Parameters]
Down
PUT Only: incrementing by 1 step (1 millisecond)
Up
PUT Only: decrementing by 1 step (1 millisecond)
Numerical Number: -250 to 250, Step: 1
PUT: setting to the specified value. / GET: indicating the current value.
The unit for this parameter is "ms".
LIPSYNCHDMIOUT1MANUAL
[PUT Command]
@MAIN:LIPSYNCHDMIOUT1MANUAL=
[Parameters]
Down
PUT Only: incrementing by 1 step (1 millisecond)
Up
PUT Only: decrementing by 1 step (1 millisecond)
Numerical Number: 0 to 250, Step: 1
PUT: setting to the specified value. / GET: indicating the current value.
The unit for this parameter is "ms".
LIPSYNCHDMIOUT2OFFSET
[PUT Command]
@MAIN:LIPSYNCHDMIOUT2OFFSET=
[Parameters]
Parameters are the same as
LIPSYNCHDMIOUT1OFFSET
LIPSYNCHDMIOUT2MANUAL
[PUT Command]
@MAIN:LIPSYNCHDMIOUT2MANUAL=
[Parameters]
Parameters are the same as
LIPSYNCHDMIOUT1MANUAL
LIPSYNCSELINFO
@MAIN:LIPSYNCSELINFO=?
Retrieving current Video Output State
[Parameters]
Analog
GET Only: indicating Analog video connection is only available (no HDMI out is in use)
HDMI1 Auto
GET Only: indicating HDMI1 output connection is effective, and the Display is compatible with Auto Lipsync
feature.
HDMI1 Manual
GET Only: indicating HDMI1 output connection is effective, and the Display is NOT compatible with Auto
Lipsync feature.
HDMI2 Auto
GET Only: indicating HDMI2 output connection is the only one in use, and the Display is compatible with Auto
Lipsync feature.
HDMI2 Manual
GET Only: indicating HDMI2 output connection is the only one in use, and the Display is NOT compatible with
Auto Lipsync feature.
LIPSYNCOFFSETINFO
@MAIN:LIPSYNCOFFSETINFO=?
Retrieving the Audio Delay Offset value that is reported by the Display compatible with Auto Lipsync feature
[Parameters]
Numerical Number: 0 to 250, Step: 1
GET Only: indicating the current value.
The unit for this parameter is "ms".
HDMIOUT
[PUT Command]
@MAIN:HDMIOUT=
Parameter
@MAIN:HDMIOUT=?
Operating & retrieving HDMI Output setting state
Initial Auto Feedback is Available
[Parameters]
Off
PUT: turining its setting state to Off (output is disabled)/ GET: indicating Off setting status.
OUT
PUT: turining its setting state to OUT (meaning output is enabled) / GET: indicating OUT setting status.
Initial Auto Feedback is Available
[Parameters]
Hall in Munich
PUT: turining its setting state to Hall in Munich / GET: indicating Hall in Munich setting status.
Hall in Vienna
PUT: turining its setting state to Hall in Vienna / GET: indicating Hall in Vienna setting status.
Chamber
PUT: turining its setting state to Chamber / GET: indicating Chamber setting status.
Cellar Club
PUT: turining its setting state to Cellar Club / GET: indicating Cellar Club setting status.
The Roxy Theatre
PUT: turining its setting state to The Roxy Theatre / GET: indicating The Roxy Theatre setting status.
The Bottom Line
PUT: turining its setting state to The Bottom Line / GET: indicating The Bottom Line setting status.
Sports
PUT: turining its setting state to Sports / GET: indicating Sports setting status.
Action Game
PUT: turining its setting state to Action Game / GET: indicating Action Game setting status.
Roleplaying Game
PUT: turining its setting state to Roleplaying Game / GET: indicating Roleplaying Game setting status.
Music Video
PUT: turining its setting state to Music Video / GET: indicating Music Video setting status.
Standard
PUT: turining its setting state to Standard / GET: indicating Standard setting status.
Spectacle
PUT: turining its setting state to Spectacle / GET: indicating Spectacle setting status.
Sci-Fi
PUT: turining its setting state to Sci-Fi / GET: indicating Sci-Fi setting status.
Adventure
PUT: turining its setting state to Adventure / GET: indicating Adventure setting status.
Drama
PUT: turining its setting state to Drama / GET: indicating Drama setting status.
Mono Movie
PUT: turining its setting state to Mono Movie / GET: indicating Mono Movie setting status.
2ch Stereo
PUT: turining its setting state to 2ch Stereo / GET: indicating 2ch Stereo setting status.
7ch Stereo
PUT: turining its setting state to 7ch Stereo / GET: indicating 7ch Stereo setting status.
Surround Decoder
PUT: turining its setting state to Surround Decoder / GET: indicating Surround Decoder setting status.
ADAPTIVEDSP
[PUT Command]
@MAIN:ADAPTIVEDSP=
[Parameters]
Off
PUT: turining its setting state to Off / GET: indicating Off setting status.
Auto
PUT: turining its setting state to Auto / GET: indicating Auto setting status.
3DCINEMA
[PUT Command]
@MAIN:3DCINEMA=
Parameter
@MAIN:3DCINEMA=?
Operating & retrieving 3D DSP setting state
[Parameters]
Off
PUT: turining its setting state to Off / GET: indicating Off setting status.
Auto
PUT: turining its setting state to Auto / GET: indicating Auto setting status.
EXSURDECODER
[PUT Command]
@MAIN:EXSURDECODER=
Parameter
@MAIN:EXSURDECODER=?
Operating & retrieving Extended Surround setting state
[Parameters]
Off
PUT: turining its setting state to Off / GET: indicating Off setting status.
Auto
PUT: turining its setting state to Auto / GET: indicating Auto setting status.
Dolby PLIIx Movie
PUT: turining its setting state to Dolby PLIIx Movie / GET: indicating Dolby PLIIx Movie setting status.
Dolby PLIIx Music
PUT: turining its setting state to Dolby PLIIx Music / GET: indicating Dolby PLIIx Music setting status.
EX/ES
PUT: turining its setting state to EX/ES / GET: indicating EX/ES setting status.
2CHDECODER
[PUT Command]
@MAIN:2CHDECODER=
[Parameters]
Dolby PL
Dolby PLII Movie
PUT: turining its setting state to Dolby PLII Movie / GET: indicating Dolby PLII Movie setting status.
Dolby PLII Music
PUT: turining its setting state to Dolby PLII Music / GET: indicating Dolby PLII Music setting status.
Dolby PLII Game
PUT: turining its setting state to Dolby PLII Game / GET: indicating Dolby PLII Game setting status.
Dolby PLIIx Movie
PUT: turining its setting state to Dolby PLIIx Movie / GET: indicating Dolby PLIIx Movie setting status.
Dolby PLIIx Music
PUT: turining its setting state to Dolby PLIIx Music / GET: indicating Dolby PLIIx Music setting status.
Dolby PLIIx Game
PUT: turining its setting state to Dolby PLIIx Game / GET: indicating Dolby PLIIx Game setting status.
DTS NEO:6 Cinema
PUT: turining its setting state to DTS NEO:6 Cinema / GET: indicating DTS NEO:6 Cinema setting status.
DTS NEO:6 Music
PUT: turining its setting state to DTS NEO:6 Music / GET: indicating DTS NEO:6 Music setting status.
PLAYBACK
[PUT Command]
@MAIN:PLAYBACK=
[Parameters]
Stop
PUT Only: change its state to Stop
Pause