Amplificateur Yamaha

Liste des commandes dans calaos installer

Fonctionne avec la serie rx

Volume X

Power on

Power off

source X

BD -> source 4
DVD -> source 5
TVSAT -> source 6
DVRBDR -> source 7
VIDEO 1 -> source 8
VIDEO 2 -> source 9
VIDEO 3 -> source 10
VIDEO 4 -> source 11
VIDEO 5 -> source 12
VIDEO 6 -> source 13
VIDEO 7 -> source 14
VIDEO 8 -> source 15
NETRADIO -> source 16
IPOD -> source 17
HDMI 1 -> source 18
HDMI 2 -> source 19
HDMI 3 -> source 20
HDMI 4 -> source 21
HDMI 5 -> source 22
HDMI 6 -> source 23
HDMI 7 -> source 24
HDMI 8 -> source 25
CD -> source 26
CDRTAPE -> source 27
TUNER -> source 28
PHONO -> source 29
MULTIIN -> source 30
APORT -> source 31
SIRIUS -> source 32
TV -> source 33
SAT -> source 34
GAME 1 -> source 35
GAME 2 -> source 36
AUX -> source 37
DOCK -> source 38
HDRADIO -> source 39
RHAPSODY -> source 40
NAPSTER -> source 41
PANDORA -> source 42
LASTFM -> source 43
FLICKR -> source 44
FAV -> source 45
SERVER -> source 46
NETWORK -> source 47
USB -> source 48
USB2 -> source 49
USB3 -> source 50
USB4 -> source 51
USB5 -> source 52
USB6 -> source 53
USB7 -> source 54
USB8 -> source 55
VCR -> source 56
AUX1 -> source 57
AUX2 -> source 58
AUX3 -> source 59
AUX4 -> source 60
AUX5 -> source 61
AUX6 -> source 62
AUX7 -> source 63
AUX8 -> source 64
BLUETOOTH -> source 65
IPODUSB -> source 66
PC -> source 67
UAW -> source 68

custom cmd

exemple

custom @MAIN:INP=HDMI1

@MAIN @ZONE2 @ZONE3

Command Details of SubUnit: MAIN
PWR
[PUT Command]
@MAIN:PWR=
[Parameters]
Standby :turining its state to Standby
On :turining its state to On
On/Standby :toggling its status between On/Standby
SLEEP
[PUT Command]
@MAIN:SLEEP=
[Parameters]
Off :turining its setting state to Off
30 min :setting to 30 min
60 min :setting to 60 min
90 min :setting to 90 min
120 min :setting to 120 min
Last :setting to the value set last
VOL
[PUT Command]
@MAIN:VOL=
[Parameters]
Down :decrementing by 1 step (0.5dB)
Up :incrementing by 1 step (0.5dB)
Down 1 dB :decrementing by 1 dB
Up 1 dB :incrementing by 1 dB
Down 2 dB :decrementing by 2 dB
Up 2 dB :incrementing by 2 dB
Down 5 dB :decrementing by 5 dB
Up 5 dB :incrementing by 5 dB
Numerical Number: -80.5 to 16.5, Step: 0.5 :setting to the specified value.
-80.5 means muting. First decimal place must be always included. Ex: 10.0, -25.0 or 0.0 etc. The unit for this parameter is "dB".
MUTE
[PUT Command]
@MAIN:MUTE=
[Parameters]
Off :turining its state to Off
Att -40 dB :attenuating by 40 dB from current volume status.
volume status.
Att -20 dB :attenuating by 20 dB from current volume status.
volume status.
On :turining its state to On
On/Off :toggling its status between On/Off
MAXVOL
[PUT Command]
@MAIN:MAXVOL=
[Parameters]
Numerical Number: -30.0 to 15.0, Step: 5.0 :setting to the specified value.
First decimal place must be always included. Ex: 10.0, -25.0 or 0.0 etc.
The unit for this parameter is "dB".
16.5: setting to the specified value.
Meaning no limit of maximum volume
The unit for this parameter is "dB".
INITVOLMODE
[PUT Command]
@MAIN:INITVOLMODE=
[Parameters]
Offturining its setting state to Off
On :turining its setting state to On
INITVOLLVL
[PUT Command]
@MAIN:INITVOLLVL=
[Parameters]
Mute :turining its setting state to Mute
Initially muted when turned on
Numerical Number: -80.0 to 16.5, Step: 0.5
setting to the specified value.
First decimal place must be always included. Ex: 10.0, -25.0 or 0.0 etc.
The unit for this parameter is "dB".
INP
[PUT Command]
@MAIN:INP=
[Parameters]
SIRIUS :selecting input SIRIUS
TUNER :selecting input TUNER
HDMI1 :selecting input HDMI1
HDMI2 :selecting input HDMI2
HDMI3 :selecting input HDMI3
HDMI4 :selecting input HDMI4
HDMI5 :selecting input HDMI5
AV1 :selecting input AV1
AV2 :selecting input AV2
AV3 :selecting input AV3
AV4 :selecting input AV4
AV5 :selecting input AV5
AV6 :selecting input AV6
V-AUX :selecting input V-AUX
AUDIO1 :selecting input AUDIO1
AUDIO2 :selecting input AUDIO2
DOCK :selecting input DOCK
iPod :selecting input iPod
Bluetooth :selecting input Bluetooth
UAW :selecting input UAW
NET :selecting input NET
Rhapsody :selecting input Rhapsody
SIRIUS InternetRadio :selecting input SIRIUS InternetRadio
Pandora :selecting input Pandora
Napster :selecting input Napster
PC :selecting input PC
NET RADIO :selecting input NET RADIO
USB :selecting input USB
iPod (USB) :selecting input iPod (USB)
DECODERSEL
[PUT Command]
@MAIN:DECODERSEL=
[Parameters]
Auto :turining its setting state to Auto
Automatically selects audio decoder. Default value.
DTS :turining its setting state to DTS
Audio decoder is fixed to DTS
SCENE
[PUT Command]
@MAIN:SCENE=
[Parameters]
Scene 1
selecting Scene 1
Scene 2
selecting Scene 2
Scene 3
selecting Scene 3
Scene 4
selecting Scene 4
SPBASS
[PUT Command]
@MAIN:SPBASS=
[Parameters]
Numerical Number: -6.0 to 6.0, Step: 0.5
setting to the specified value.
First decimal place must be always included. Ex: 3.0, -4.0
The unit for this parameter is "dB".
SPTREBLE
[PUT Command]
@MAIN:SPTREBLE=
[Parameters]
Parameters are the same as
SPBASS
PUREDIRMODE
[PUT Command]
@MAIN:PUREDIRMODE=
[Parameters]
Off :turining its setting state to Off
On :turining its setting state to On
ADAPTIVEDRC
[PUT Command]
@MAIN:ADAPTIVEDRC=
[Parameters]
Off :turining its setting state to Off
Auto :turining its setting state to Auto
LIPSYNCMODE
[PUT Command]
@MAIN:LIPSYNCMODE=
[Parameters]
Manual :turining its setting state to Manual
About "Manual" setting of Lipsync Mode: When selecting "Manual" here, the audio delay value can be
manually set. The effective setting of the audio delay value has some dependencies as follows. In case of
using Analog Video Output only (no HDMI connection is active), audio delay value set by "@MAIN:ANLGOUT"
command is effective. In case that HDMI OUT1 is in active connection, the value set by
"@MAIN:HDMIOUT1MANUAL" command works. Else if HDMI OUT2 is the only one activated, the setting by
"@MAIN:HDMIOUT2MANUAL" is enabled.
Auto :turining its setting state to Auto
About Lipsync Mode "Auto": Basically, Audio Delay value has 5 different settings internally according to "Video
Output State (5 Status available)". And the 5 different status of "Video Output State" is determined by the
combination of two states of "Display's state of compatibility/incompatibility with Auto Lipsync feature" and
"Current effective HDMI output state (on the receiver)", which means 4 status, plus a status of "Analog Video
Out only in use", summing up to 5 in total. The "Auto" setting of Lipsync Mode is to dynamically change the
Audio Delay value corresponding to a specific status of Video Output State. "Video Output State" can be
retrieved with a command of "@MAIN:SELINFO", and you can set the effective Audio Delay value according to
respective Video Output status by these commands as following;
When "@MAIN:SELINFO=Analog": the audio delay can be set by "@MAIN:ANLGOUT" command
When "@MAIN:SELINFO=HDMI1 Auto" (meaning TV compatible with Auto Lipsync and HDMI OUT1 is
effective): the audio delay can be set by "@MAIN:HDMIOUT1OFFSET" command
When "@MAIN:SELINFO=HDMI1 Manual" (meaning TV incompatible with Auto Lipsync and HDMI OUT1 is
effective): the audio delay can be set by "@MAIN:HDMIOUT1MANUAL" command
When "@MAIN:SELINFO=HDMI2 Auto" (meaning TV compatible with Auto Lipsync and HDMI OUT 2 is the
only one in effective): the audio delay can be set by "@MAIN:HDMIOUT2OFFSET" command
When "@MAIN:SELINFO=HDMI2 Manual" (meaning TV incompatible with Auto Lipsync and HDMI OUT 2 is
the only one in effective): the audio delay can be set by "@MAIN:HDMIOU21MANUAL" command
LIPSYNCANLGOUT
[PUT Command]
@MAIN:LIPSYNCANLGOUT=
[Parameters]
Down
incrementing by 1 step (1 millisecond)
Up
decrementing by 1 step (1 millisecond)
Numerical Number: 0 to 250, Step: 1
setting to the specified value.
The unit for this parameter is "ms".
LIPSYNCHDMIOUT1OFFSET
[PUT Command]
@MAIN:LIPSYNCHDMIOUT1OFFSET=
[Parameters]
Down
incrementing by 1 step (1 millisecond)
Up
decrementing by 1 step (1 millisecond)
Numerical Number: -250 to 250, Step: 1
setting to the specified value.
The unit for this parameter is "ms".
LIPSYNCHDMIOUT1MANUAL
[PUT Command]
@MAIN:LIPSYNCHDMIOUT1MANUAL=
[Parameters]
Down
incrementing by 1 step (1 millisecond)
Up
decrementing by 1 step (1 millisecond)
Numerical Number: 0 to 250, Step: 1
setting to the specified value.
The unit for this parameter is "ms".
LIPSYNCHDMIOUT2OFFSET
[PUT Command]
@MAIN:LIPSYNCHDMIOUT2OFFSET=
[Parameters]
Parameters are the same as
LIPSYNCHDMIOUT1OFFSET
LIPSYNCHDMIOUT2MANUAL
[PUT Command]
@MAIN:LIPSYNCHDMIOUT2MANUAL=
[Parameters]
Parameters are the same as
LIPSYNCHDMIOUT1MANUAL
HDMIOUT
[PUT Command]
@MAIN:HDMIOUT=
[Parameters]
Off :turining its setting state to Off (output is disabled)
OUT :turining its setting state to OUT (meaning output is enabled)
Initial Auto Feedback is Available
[Parameters]
Hall in Munich :turining its setting state to Hall in Munich
Hall in Vienna :turining its setting state to Hall in Vienna
Chamber :turining its setting state to Chamber
Cellar Club :turining its setting state to Cellar Club
The Roxy Theatre :turining its setting state to The Roxy Theatre
The Bottom Line :turining its setting state to The Bottom Line
Sports :turining its setting state to Sports
Action Game :turining its setting state to Action Game
Roleplaying Game :turining its setting state to Roleplaying Game
Music Video :turining its setting state to Music Video
Standard :turining its setting state to Standard
Spectacle :turining its setting state to Spectacle
Sci-Fi :turining its setting state to Sci-Fi
Adventure :turining its setting state to Adventure
Drama :turining its setting state to Drama
Mono Movie :turining its setting state to Mono Movie
2ch Stereo :turining its setting state to 2ch Stereo
7ch Stereo :turining its setting state to 7ch Stereo
Surround Decoder :turining its setting state to Surround Decoder
ADAPTIVEDSP
[PUT Command]
@MAIN:ADAPTIVEDSP=
[Parameters]
Off :turining its setting state to Off
Auto :turining its setting state to Auto
3DCINEMA
[PUT Command]
@MAIN:3DCINEMA=
Parameter
@MAIN:3DCINEMA=?
Operating & retrieving 3D DSP setting state
[Parameters]
Off :turining its setting state to Off
Auto :turining its setting state to Auto
EXSURDECODER
[PUT Command]
@MAIN:EXSURDECODER=
Parameter
@MAIN:EXSURDECODER=?
Operating & retrieving Extended Surround setting state
[Parameters]
Off :turining its setting state to Off
Auto :turining its setting state to Auto
Dolby PLIIx Movie :turining its setting state to Dolby PLIIx Movie
Dolby PLIIx Music :turining its setting state to Dolby PLIIx Music
EX/ES :turining its setting state to EX/ES
2CHDECODER
[PUT Command]
@MAIN:2CHDECODER=
[Parameters]
Dolby PL
Dolby PLII Movie :turining its setting state to Dolby PLII Movie
Dolby PLII Music :turining its setting state to Dolby PLII Music
Dolby PLII Game :turining its setting state to Dolby PLII Game
Dolby PLIIx Movie :turining its setting state to Dolby PLIIx Movie
Dolby PLIIx Music :turining its setting state to Dolby PLIIx Music
Dolby PLIIx Game :turining its setting state to Dolby PLIIx Game
DTS NEO:6 Cinema :turining its setting state to DTS NEO:6 Cinema
DTS NEO:6 Music :turining its setting state to DTS NEO:6 Music
PLAYBACK
[PUT Command]
@MAIN:PLAYBACK=
[Parameters]
Stop : change its state to Stop
Pause